Please remove and update “(1) ,(2)and (3)” in u-boot-2009.08/drivers/mtd/spi/imx\_spi\_nor\_m25pxx.c .

1. In struct imx\_spi\_flash\_params.

Remove

~~#ifdef CONFIG\_ADVANTECH~~

~~u32 idcode2;~~

~~u32 idcode3;~~

~~#endif~~

1. In struct imx\_spi\_flash.

Remove


~~#ifdef CONFIG\_ADVANTECH~~

~~.idcode2 = 0x16,~~

~~.idcode3 = 0xEF,~~

~~#endif~~


Old version New version



(3) Please follow the new version and update it.

struct spi\_flash \*spi\_flash\_probe(unsigned int bus, unsigned int cs, unsigned int max\_hz, unsigned int spi\_mode)

Old version New version



Download the new spi driver (imx\_spi\_nor\_m25pxx.c).

<https://www.dropbox.com/s/julel9ttrb3vvh9/imx_spi_nor_m25pxx.c?dl=0>

Please check your uboot(2009.08) and update new version. (SPI)