advanech.jpg

Functional Requirement

Plugin sample code for WISE-Agent Handshake protocol

**Revision History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Revision** | **Date** | **Notes** | **Owner** |
| 1.0 | 2018/05/07 | Draft for review | Wang.yu |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Project (\*)** | Plugin sample code for WISE-Agent Handshake protocol | **Apply Date (\*)** | | 2018/5/7 | |
| **Customer (\*)** | 晶创 | **Business (\*)** | | NRE - # ? | |
| **PM (\*)** | Wang.yu | **AE (\*)** | | - | |
| **Platform (\*)** | - | **OS (\*)** | | Windows | |
| **Peripheral** | **Name** | **Purpose** | | | |
|  |  | | | |
|  |  | | | |
| **User /**  **Functional Requirements** | **Description** | | **Evaluate Solution** | | **Version** |
| Plugin sample code for WISE-Agent Handshake protocol | |  | | V1.0 |
|  | |  | |  |
|  | |  | |  |
|  | |  | |  |
|  | |  | |  |
| **Others** | | | | | |
| 1. 使用EI-Agent傳送符合RMM handshake protocol資料，這點gateway sample及handshake protocol； 2. RMM Data Worker接收数据；可以将每个PLC识别成一个独立的Device （具备相同的Parent DID = EI-agent‘s did） 3. 每个PLC可以主动决定何时传送资料，每次只传送部分Sensor的资料；   备注：周三下午16:00对西安RD进行一次针对这个Sample的技转说明 | | | | | |
|  | | | | | |

**(\*): Must**