

User / Functional Requirement

Modbus TCP Slave for POC

( For Reyax LoRa Sensor Node only)

**Revision History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Revision** | **Date** | **Notes** | **Owner** |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Project (\*)** | Modbus TCP Slave for POC | **Apply Date (\*)** | 2018/08/16 |
| **Customer (\*)** | Hyundai | **Business (\*)** | NRE |
| **PM (\*)** | Brook.Lee | **AE (\*)** | Ray.Liu |
| **Platform** | UTX-3117 | **OS (\*)** | Ubuntu 16.04 x64 |
| **Peripheral** | **Name** | **Purpose** |
|  |  |
|  |  |
| **User /****Functional Requirements** | **Description** | **Evaluate Solution** | **Version** |
| SCADA would get LoRa node sensor data from UTX-3117 by Modbus TCP  | Modbus TCP Slave | 1.0 |
| Fixed LoRa sensor data as below picture. | Hardcode for this POC | 1.0 |
|  |  |  |
|  |  |  |
|  |  |  |
| **Others** |
| Architecture of this POC demo: |
|  |

**(\*): Must**