**EWM FAQ**

|  |  |  |  |
| --- | --- | --- | --- |
| **Category** | EWM | **Date** | 2020/04/23 |
| **Keyword** | LTE 4G network ,UTX-3117,EWM-C117FL0XE,Linux OS, Fedora 31  |

* **Question:**

How to establish 4G cellular network with EWM-C117FL0XE module on Fedora OS?

* **Instructions :**

Step 1

Confirm if the network interface has generated in network setting

* Enter “ifconfig” command on terminal



Step 2

Enter to GUI network setting to create your own connection

 

Step 3

Choose your provider’s country or region



Step 4

Select your provider from list (if the provider is not appeared in list, please input by yourself)



Step 5

Double Confirm if the APN is used for your sim card or not



Step 6

If you would like to auto connect when system boots up, please tick up following option in general section



Step 7

Save your setting and enable your network connection on mobile broadband feature, then do ping test to confirm connection status



Step 8

If the mobile broadband cannot control by GUI button, please try to restart the mobile broadband service by following command to recovery it

* Enter “ sudo systemctl restart ModemManager” command on terminal

