**How to Setup Network with AIW-341**


**Prerequisite**


* MIO-5393 and setup Windows 10 on it
* AIW-341 module.

**Install Driver**

* Device driver


Please run the installer “FbUSBDeviceSetup.exe” (version v2.1.2.5) and follow the prompt to install driver.





**Check Device**


After driver installed, you will see the snapshot as below.



**Function Test**

* Speed test

This is only for reference.




* Reliability

Observe the ping test at least 6 hours.

* AT command

1. Check the number of COM port with AIW-344 in device manager.



1. Access to AT command through terminal like putty.

Please make setting as below:

* + Baud Rate “9600”
  + Data bits "8"
  + Stop bits "1"
  + Parity "None"
  + Flow Control "None"

