**AIW FAQ**

|  |  |  |  |
| --- | --- | --- | --- |
| **Category** | ePaper Manager, EPD-230,EPD-332, WISE-3240 | **Date** | 2021/9/17 |
| **Keyword** | ePaper Manager, EPD-230, EPD-332, EPD-662, WISE-3240 |

* **Question:**

EPD FAQ - How to modify TX power, Channel, status report period and data request period?

* **Steps:**

In the WISE-3240, you can modify TX power and Channel.

In the EPD-230 and EPD-332, you can modify status report period and data request period.

Step 1: Log in ePaper Manager and click Device list

Step 2: Click “Get/Set” to the configuration web page and select the tag to modify status report period and data request period.



Step 3: Click “SenHub”



Step 4: Finding “data-request-period” to modify data request period.



Step 5: Modify the value and the unit is second.



Step 6: Finding “state-report-period” to modify data request period.



Step 7: Modify the value and the unit is second.



Step 8: Regarding modify TX power and Channel, select router’s “get/set”



Step 9: Select IoT GW



Step 10: Modify TX power, please select “tx-level-r”



Step 11: Change the value and the unit is dBm.



Step 12: Go back to select “Channel”



Step 13: You can change the WISE-3240 Channel. Regarding how to select the channel, please reference the other document “EPD Deploy Guide - How to estimate the deployment of ePaper Manager system.pdf”

