**EWM FAQ**

|  |  |  |  |
| --- | --- | --- | --- |
| **Category** | EWM | **Date** | 2020/06/18 |
| **Keyword** | EWM-C148FL02E,windows 10 OS (Version1809),UTX-3117 | | |


* **Question:**

How to establish LTE cellular network with EWM-C148FL02E on windows 10 OS x86 platform?

* **Instructions :**

Step 1

Insert EWM-C148FL02E module into mini PCI-E slot and both of Main and Aux has connected antenna cables already.




Step 2


Download windows driver package by following URL and install on your OS

<https://www.dropbox.com/sh/cdgxv4401otjk7l/AAAzo73R-bU-lgz7nIJyWazQa/4G/CAT4/C148/Driver/Windows?dl=0>

Step 3

Enter to Setting section and enable cellular mode for establishing cellular connection





Step 4

After enabling, the cellular function will auto-search 3G/4G signal around your place to establish connection.

