**EWM FAQ**

|  |  |  |  |
| --- | --- | --- | --- |
| **Category** | EWM | **Date** | 2019/11/19 |
| **Keyword** | EWM-C117FL02E ,4G/LTE Connection | | |

* **Question:**

How to connect 4G/LTE with EWM-C117FL02E in RNDIS mode?

* **Instructions :**

Step 1

Download related utilities and driver from following link and decompress the file at local device

<https://1drv.ms/u/s!AmPTlw75mrwLgzICSmT1IaNxFiEI>




Step 2

Install cellular module on your device and make sure RNDIS driver has installed successfully




Step 3

Enter to device manager and ensure the u-blox USB modem interface has generated




Step 4

Execute m-center utility to configure related setting




Step 5

After selecting Com port, press connect button for connecting, then press “Get info” button to acquire modem information




Step 6

Input SIM card’s PIN Code




**<Note>**

Disable your sim card’s pin code to avoid inputting every time when you logon system




Step 7

Switch to AT terminal mode and select specific AT group (**Set\_APN**) and input Commands orderly.



Step 8

If your SIM card already include username and password, please select “**Set\_APN\_user/pwd**” AT group and change APN/USERNAME/PASSWORD before sending commands.



Step 9

Close AT terminal session and exit m-center utility, then reboot system for establishing RNDIS connection automatically.

Step 10

After above configurations, you will see the connection is established to browse internet as usual.

