**How to Setup Network with AIW-342**

**Prerequisite**

* MIO-5373 and setup Windows 10 on it

**Install Driver**

* Device driver


Please run the installer “TelitWHQLDriversxXX.msi” after extract the file “Telit\_Windows\_10\_WHQL\_Drivers\_Installer\_2.09.0002.zip” and follow the prompt to install driver.

* AT command utility

Please run the installer “Setup\_TATC\_3.3.1\_\_XFP\_3.2.2.msi” after extract the file “Telit\_AT\_Controller\_r3.3.1\_XFP\_3.2.2.zip” and follow the prompt to install utility.

**Check Device**


After driver installed, you will see the snapshot as below.



**Function Test**

* Speed test

This is only for reference.



* Reliability

Observe the ping test at least 6 hours.

* AT command

Open the “Telit AT Controller” utility and setting as below, then input the AT command to test.

