**How to Setup Network with AIW-342**

**on Ubuntu**

**Prerequisite**

* EPC-R7200 and setup Ubuntu 18.04 from nVidia BSP on it
* Tarball file “aiw-342-peer-config.tar.bz2”

**Test**

* Stop modem manager

# sudo service ModemManager stop

* Copy configuration file

decompress the tarball “aiw-342-peer-config.tar.bz2”

# tar jxvf “aiw-342-peer-config.tar.bz2”

Copy all files to /etc/ppp/peers

# sudo cp aiw-342-peer-config/\* /etc/ppp/peers/

* Open the file “aiw-342-chat” and modify the APN

# sudo vi /etc/ppp/peers/aiw-342-chat

To fill the string of your APN in the below red rectangle.



* Dial out

# sudo pppd call aiw-342 &





* Check network connection

# ping -c 3 -I ppp0 8.8.8.8

