**WISE-EC FAQ**

|  |  |  |  |
| --- | --- | --- | --- |
| **Category** | WISE-EC | **Date** | 2018/01/16 |
| **Keyword** | WISE-EC, WISE-1520,WISE-3610  |

* **Question:**

How to verify the wifi profile is configured successfully when connecting wise-1520 in Station mode?

* **Instructions :**

Step 1

Ensure all of equipment already Set up at your side



Step 2

 Refer to our internal detail SOP to make sure all of steps configure proper

<https://drive.google.com/open?id=1YvPKC3P9rDuzgJLeud_mQx3xlnKLztsL>

Step 3

[mobile\_Hotspot]

When you login to wise-1520 setting webpage, please ensure the profile can be created so that can connected proper in station mode

 

Step 4

 Set into AP mode



Step 5

 Press reset button and check the output message on console and the connection can be established successfully





[Wise 3610]







* **Issue Clarification:**
1. We don’t have wise-3620 at our side that is the reason why I test on wise-3610.

the model is difference, but it may not the root cause of this problem on your testing. <the only different is with/without LoRa module between wise-3610 and wise-3620>

1. If the connection still cannot connect after above instructions, please record a video during your testing for further investigation.