**EWM FAQ**

|  |  |  |  |
| --- | --- | --- | --- |
| **Category** | EWM | **Date** | 2021/04/22 |
| **Keyword** | AIW-344FQ(EWM-C148FL02E),windows 10 OS (Version1809),UTX-3117 | | |


* **Question:**

How to establish LTE cellular network with AIW-344FQ(EWM-C148FL02E) on windows 10 OS x86 platform?

* **Instructions :**

Step 1

Insert AIW-344FQ(EWM-C148FL02E) module into mini PCI-E slot and both of Main and Aux has connected antenna cables already




Step 2

Download windows driver package by following URL and install on your OS

<https://1drv.ms/u/s!AvzLe5sr2qg2g8kKnlENkfCyqiOLRg?e=szaQdI>

Step 3


Enter to Setting section and enable cellular mode for establishing cellular connection




Step 4


With specific sim card, it must enter APN setting, username and password in advance

* Click advance option to add APN profile







* Add related configuration and apply it



Step 5

After enabling, the cellular function will auto-search 3G/4G signal around your place to establish connection





Step 6

Access the internet by browser and ensure if the webpage can show normal or not

