**AIW(EWM) FAQ**

|  |  |  |  |
| --- | --- | --- | --- |
| **Category** | AIW | **Date** | 2022/02/08 |
| **Keyword** | AIW-166, Windows 10 Enterprise LTSC(version 1809) |

* **Question:**

How to fix yellow bang(error code 10) issue on AIW-166(Intel WiFi-6E AX210 160MHz)?





* **Instructions :**

Step 1

Download the newer wireless adapter driver version 22.110.1 or above from Windows official website. <https://www.intel.com.tw/content/www/tw/zh/download/19351/windows-10-and-windows-11-wi-fi-drivers-for-intel-wireless-adapters.html?wapkw=19351>

Step 2

 Run the .exe file to install the driver 22.110.1, then reboot the PC.

Step 3

 After PC reboot, yellow bang(error code 10) issue has disappeared and AIW-166 works well.



2.4GHz SSID:



5GHz SSID:



\*Note: If the issue still existed after upgraded the newer driver, please try to disable and enable the Wi-Fi adapter then reboot the PC once again.

Platform information:

